{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":91,"n_cols":3,"rows_kept":91,"cut":false,"hidden":false,"merged":[]}
["id","partName","audioClipName"]
[1,"充气套管","3.1 充气套管"]
[2,"充气套管","3.2 充气套管"]
[3,"O型环","3.3 O型环"]
[4,"均压环","3.4 均压环"]
[5,"绝缘套管","3.5 绝缘套管"]
[6,"密封垫","3.6 密封垫"]
[7,"密封盖","3.7 密封盖"]
[8,"放气螺栓","3.8 放气螺栓"]
[9,"充气套管连接座","3.9 充气套管连接座"]
[10,"导电杆","3.10 导电杆"]
[11,"开槽盖","3.11 开槽盖"]
[12,"油枕及弹簧","3.12 油枕及弹簧"]
[13,"设备线接","3.13 设备线接"]
[14,"充气套管","3.14 充气套管"]
[15,"O型环","3.15 O型环"]
[16,"均压环","3.16 均压环"]
[17,"套管","3.17 套管"]
[18,"密封垫","3.18 密封垫"]
[19,"密封盖","3.19 密封盖"]
[20,"充气套管连接座","3.20 充气套管连接座"]
[21,"放气螺栓","3.21 放气螺栓"]
[22,"导电杆","3.22 导电杆"]
[23,"开槽盖","3.23 开槽盖"]
[24,"油枕及弹簧","3.24 油枕及弹簧"]
[25,"接线端子","3.25 接线端子"]
[26,"主体","3.26 主体"]
[27,"压力表","3.27 压力表"]
[28,"电流互感器","3.28 电流互感器"]
[29,"机构箱","3.29 机构箱"]
[30,"端子排安装导轨","3.30 端子排安装导轨"]
[31,"拐臂","3.31 拐臂"]
[32,"灯","3.32 灯"]
[33,"盖板","3.33 盖板"]
[34,"线路板","3.34 线路板"]
[35,"辅助开关","3.35 辅助开关"]
[36,"延时继电器","3.36 延时继电器"]
[37,"空开","3.37 空开"]
[38,"端子排","3.38 端子排"]
[39,"航空插头底座","3.39 航1空插头底座"]
[40,"连杆","3.40 连杆"]
[41,"连杆轴","3.41 连杆轴"]
[42,"连板","3.42 连板"]
[43,"外壳","3.43 外壳"]
[44,"柜门","3.44 柜门"]
[45,"机构箱固定板","3.45 机构箱固定板"]
[46,"断路器","3.46 断路器"]
[47,"断路器内部","3.47 断路器内部"]
[48,"高压触头导向柱","3.48 高压触头导向柱"]
[49,"接线板","3.49 接线板"]
[50,"接线板","3.50 接线板"]
[51,"静触头","3.51 静触头"]
[52,"静触头","3.52 静触头"]
[53,"动触头","3.53 动触头"]
[54,"动触头","3.54 动触头"]
[55,"阀体外壳","3.55 阀体外壳"]
[56,"拐臂","3.56 拐臂"]
[57,"铰链支座","3.57 铰链支座"]
[58,"液压驱动杆​​","3.58 液压驱动杆​​"]
[59,"主阀杆","3.59 主阀杆"]
[60,"固定座","3.60 固定座"]
[61,"外壳","3.61 外壳"]
[62,"舱盖","3.62 舱盖"]
[63,"舱盖","3.63 舱盖"]
[64,"舱盖","3.64 舱盖"]
[65,"检修盖","3.65 检修盖"]
[66,"液压操动机构","3.66 液压操动机构"]
[67,"液压操作外壳","3.67 液压操作外壳"]
[68,"碟簧","3.68 碟簧"]
[69,"偏心轴承","3.69 偏心轴承"]
[70,"储能机构","3.70 储能机构"]
[71,"储能电机","3.71 储能电机"]
[72,"油泵密封盖","3.72 油泵密封盖"]
[73,"泄压阀","3.73 泄压阀"]
[74,"排油阀","3.74 排油阀"]
[75,"活塞","3.75 活塞"]
[76,"控制模块","3.76 控制模块"]
[77,"换向阀","3.77 换向阀"]
[78,"分闸线圈","3.78 分闸线圈"]
[79,"分闸线圈","3.79 分闸线圈"]
[80,"合闸线圈","3.80 合闸线圈"]
[81,"控制模块","3.81 控制模块"]
[82,"防慢分装置","3.82 防慢分装置"]
[83,"通气阀","3.83 通气阀"]
[84,"分合闸指示器","3.84 分合闸指示器"]
[85,"辅助开关","3.85 辅助开关"]
[86,"储能模块","3.86 储能模块"]
[87,"传动杆","3.87 传动杆"]
[88,"操动机构主体","3.88操动机构主体"]
[89,"密度继电器","3.89 密度继电器"]
[90,"水泥台","3.90 水泥台"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}