{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":62,"n_cols":1,"rows_kept":62,"cut":false,"hidden":false,"merged":[]}
["moveName"]
["动触头"]
["加热器主体"]
["二次插头"]
["面板"]
["线"]
["二次元件面板"]
["输出轴"]
["合闸传动机构"]
["辅助开关连杆"]
["辅助开关拐臂"]
["辅助开关本体"]
["辅助开关"]
["分闸按钮"]
["分闸线圈"]
["分闸半轴"]
["分闸扇形板"]
["连杆"]
["分闸质子"]
["拐臂"]
["分闸缓冲器"]
["分合闸指示牌连杆"]
["分合闸固定轴"]
["连接弹簧"]
["分合闸指示牌"]
["计数器"]
["储能行程开关"]
["储能指示牌固定轴"]
["储能指示牌"]
["储能轴"]
["储能拐臂"]
["合闸弹簧"]
["合闸挚子"]
["合闸半轴"]
["合闸按钮"]
["合闸线圈"]
["行程开关"]
["驱动销"]
["滑块"]
["滚轮"]
["储能传动轮"]
["储能指示驱动板"]
["合闸凸轮"]
["传动链条"]
["大链轮"]
["端子排"]
["转子"]
["定子"]
["轴"]
["电机外壳"]
["电机输出轴"]
["减速器齿轮"]
["减速机外壳"]
["小链轮"]
["涡轮"]
["手动储能蜗杆"]
["手动储能机构外壳"]
["手车位置闭锁装置"]
["断路器外壳"]
["输出拐臂"]
["输出连杆"]
["连板"]