{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":127,"n_cols":1,"rows_kept":127,"cut":false,"hidden":false,"merged":[]}
["moveName"]
["拆下接线端子"]
["拆下均压环"]
["拆下密封盖"]
["拆下密封垫"]
["拆下开槽盖"]
["拆下油枕及弹簧"]
["拆下导电杆"]
["拆下绝缘套管"]
["拆下充气套管连接座"]
["拆下O型环"]
["拆下支撑导电座"]
["拆下变直机构拐臂"]
["拆下静弧触头"]
["拆下静主触头"]
["拆下端部固定板"]
["拆下并联电容器"]
["拆下其他绝缘附件"]
["拆下动端触头压气缸"]
["拆下喷口"]
["拆下压气缸"]
["拆下中间触头"]
["拆下动触头"]
["拆下铰链支座"]
["拆下固定座"]
["拆下主阀杆"]
["拆下阀体外壳"]
["拆下压力表"]
["拆下线圈"]
["拆下电流互感器"]
["拆下密度继电器"]
["拆下外壳"]
["拆下盖板"]
["拆下分闸换向阀二次接线"]
["拆下合闸换向阀二次接线"]
["拆下控制模块"]
["拆下储能电机"]
["拆下油泵密封盖"]
["拆下偏心轴承"]
["拆下活塞"]
["拆下防慢分装置"]
["拆下储能模块"]
["拆下泄压阀"]
["拆下通气阀"]
["拆下排油阀"]
["拆下辅助开关"]
["拆下碟簧"]
["拆下传动杆"]
["拆下分合闸指示器"]
["拆下操动机构主体"]
["拆下液压操作机构外壳"]
["拆下柜门"]
["拆下灯"]
["拆下空开"]
["拆下延时继电器"]
["拆下线路板"]
["拆下端子排安装导轨"]
["拆下端子排"]
["拆下行空插头底座"]
["拆下拐臂"]
["拆下连杆"]
["拆下连板"]
["拆下连杆轴"]
["拆下机构箱固定板"]
["安装接线端子"]
["安装均压环"]
["安装密封盖"]
["安装密封垫"]
["安装开槽盖"]
["安装油枕及弹簧"]
["安装导电杆"]
["安装绝缘套管"]
["安装充气套管连接座"]
["安装O型环"]
["安装支撑导电座"]
["安装变直机构拐臂"]
["安装静弧触头"]
["安装静主触头"]
["安装端部固定板"]
["安装并联电容器"]
["安装其他绝缘附件"]
["安装动端触头压气缸"]
["安装喷口"]
["安装压气缸"]
["安装中间触头"]
["安装动触头"]
["安装铰链支座"]
["安装固定座"]
["安装主阀杆"]
["安装阀体外壳"]
["安装压力表"]
["安装线圈"]
["安装电流互感器"]
["安装密度继电器"]
["安装外壳"]
["安装盖板"]
["安装分闸换向阀二次接线"]
["安装合闸换向阀二次接线"]
["安装控制模块"]
["安装储能电机"]
["安装油泵密封盖"]
["安装偏心轴承"]
["安装活塞"]
["安装防慢分装置"]
["安装储能模块"]
["安装泄压阀"]
["安装通气阀"]
["安装排油阀"]
["安装辅助开关"]
["安装碟簧"]
["安装传动杆"]
["安装分合闸指示器"]
["安装操动机构主体"]
["安装液压操作机构外壳"]
["安装柜门"]
["安装灯"]
["安装空开"]
["安装延时继电器"]
["安装线路板"]
["安装端子排安装导轨"]
["安装端子排"]
["安装行空插头底座"]
["安装拐臂"]
["安装连杆"]
["安装连板"]
["安装连杆轴"]
["安装机构箱固定板"]