{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":149,"n_cols":3,"rows_kept":149,"cut":false,"hidden":false,"merged":[]}
["id","partName","audioClipName"]
[1,"扇叶","1.1"]
[2,"叶片","1.2"]
[3,"桨毂罩壳顶盖",1.3]
[4,"桨毂罩壳",1.4]
[5,"桨毂",1.5]
[6,"压板",1.6]
[7,"变桨减速机",1.7]
[8,"皮带",1.8]
[9,"桨毂体",1.9]
[10,"顶盖支架","1.10"]
[11,"轴承外圈",1.11]
[12,"轴承内圈",1.12]
[13,"变桨限位器组",1.13]
[14,"变桨驱动器",1.14]
[15,"变桨润滑油泵",1.15]
[16,"润滑油管路",1.16]
[17,"桨毂",1.17]
[18,"轮毂",1.18]
[19,"锁定套",1.19]
[20,"动轴","1.20"]
[21,"轴承挡环",1.21]
[22,"轴承压板固定",1.22]
[23,"轴承内圈",1.23]
[24,"主轴承滚子组",1.24]
[25,"轴承支撑环",1.25]
[26,"刹车卡钳",1.26]
[27,"滑环",1.27]
[28,"定轴",1.28]
[29,"液压锁定端盖",1.29]
[30,"锁定销","1.30"]
[31,"锁定销",1.31]
[32,"活塞耐磨环",1.32]
[33,"活塞油封",1.33]
[34,"活塞",1.34]
[35,"密封环",1.35]
[36,"活塞套",1.36]
[37,"端盖",1.37]
[38,"顶丝",1.38]
[39,"活塞密封",1.39]
[40,"透明隔板","1.40"]
[41,"定子铁芯",1.41]
[42,"绕组",1.42]
[43,"转子",1.43]
[44,"密封支撑环",1.44]
[45,"密封",1.45]
[46,"转子盖板",1.46]
[47,"机舱",1.47]
[48,"机舱顶部设备",1.48]
[49,"航空警示灯",1.49]
[50,"风速计","1.50"]
[51,"风向仪",1.51]
[52,"防雷杆",1.52]
[53,"机舱外壳",1.53]
[54,"机舱外罩",1.54]
[55,"机舱内部",1.56]
[56,"风机",1.57]
[57,"风机左",1.58]
[58,"送风管左",1.59]
[59,"垫圈左","1.60"]
[60,"通风波纹管左",1.61]
[61,"风机右",1.62]
[62,"送风管右",1.63]
[63,"垫圈右",1.64]
[64,"通风波纹管右",1.65]
[65,"风机底座左",1.66]
[66,"风机底座右",1.67]
[67,"悬臂吊",1.68]
[68,"电动吊机",1.69]
[69,"附臂","1.70"]
[70,"主臂",1.71]
[71,"悬臂吊立柱",1.72]
[72,"底座外壳",1.73]
[73,"底座外壳",1.75]
[74,"上支架",1.76]
[75,"底座人孔门",1.77]
[76,"机舱步梯",1.78]
[77,"底座人孔门盖板",1.79]
[78,"底座步梯","1.80"]
[79,"底座",1.81]
[80,"底座设备",1.82]
[81,"机舱控制柜",1.83]
[82,"发电机冷却控制装置",1.84]
[83,"润滑油供油装置",1.85]
[84,"液压站",1.86]
[85,"底座地板",1.87]
[86,"底座地板门",1.88]
[87,"塔筒爬梯",1.89]
[88,"底座地板","1.90"]
[89,"刹车卡钳",1.91]
[90,"机舱平台",1.92]
[91,"安全门",1.93]
[92,"机舱地板舱门",1.94]
[93,"液压蓄能器",1.95]
[94,"灭火器",1.96]
[95,"盖板",1.98]
[96,"偏航系统","1.149"]
[97,"偏航电机",1.74]
[98,"偏航轴承",1.99]
[99,"偏航轴承外圈","1.100"]
[100,"偏航轴承内圈",1.101]
[101,"轴承密封",1.102]
[102,"偏航轴承",1.103]
[103,"刹车盘",1.104]
[104,"偏航系统",1.97]
[105,"塔筒",1.105]
[106,"上段塔筒",1.106]
[107,"中段塔筒",1.107]
[108,"中下段塔筒",1.108]
[109,"下段塔筒",1.109]
[110,"护栏","1.110"]
[111,"线缆敷设",1.111]
[112,"楼板A",1.112]
[113,"接线柜",1.113]
[114,"升降电梯",1.114]
[115,"楼板B",1.115]
[116,"塔筒底部舱门",1.116]
[117,"塔底控制柜",1.117]
[118,"就地控制箱",1.118]
[119,"灭火器",1.119]
[120,"塔筒","1.120"]
[121,"风机步梯",1.121]
[122,"散热器护栏",1.122]
[123,"整流器",1.123]
[124,"空气水冷",1.124]
[125,"风机底座",1.125]
[126,"箱变",1.126]
[127,"高压室门",1.127]
[128,"高压室内部",1.128]
[129,"避雷器运行监测器",1.129]
[130,"接地远方开关","1.130"]
[131,"合闸显示分闸按钮",1.131]
[132,"铭牌A",1.132]
[133,"操作手柄",1.133]
[134,"低压室门",1.134]
[135,"低压室内部",1.135]
[136,"接地柜",1.136]
[137,"AB线电压",1.137]
[138,"BC线电压",1.138]
[139,"CA线电压",1.139]
[140,"A相电流","1.140"]
[141,"B相电流",1.141]
[142,"C相电流",1.142]
[143,"新能源测控装置",1.143]
[144,"分闸显示合闸按钮",1.144]
[145,"合闸显示分闸按钮",1.145]
[146,"接地远方开关",1.146]
[147,"铭牌B",1.147]
[148,"高压室外壳",1.148]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}