{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":103,"n_cols":1,"rows_kept":103,"cut":false,"hidden":false,"merged":[]}
["moveName"]
["拆下防爆盖"]
["拆下上接线板"]
["拆下静触头"]
["拆下静弧触头"]
["拆下泄弧剂"]
["拆下绝缘拉杆"]
["拆下法兰（外部端子接线端）"]
["拆下灭弧室"]
["拆下灭弧室瓷套"]
["拆下压气缸"]
["拆下下接线板"]
["拆下连接轴销"]
["拆下立柱瓷套下法兰"]
["拆下绝缘子"]
["拆下绝缘瓷套"]
["拆下接线板"]
["拆下静主触头"]
["拆下操作箱柜门"]
["拆下复位弹簧"]
["拆下合闸线圈"]
["拆下分闸线圈"]
["拆下限位开关"]
["拆下电机二次接线"]
["拆下储能电机"]
["拆下辅助开关"]
["拆下储能凸轮"]
["拆下小齿轮"]
["拆下齿轮轴"]
["拆下弹簧输出轴"]
["拆下传动齿轮"]
["拆下合闸脱扣器"]
["拆下合闸掣子"]
["拆下分闸掣子"]
["拆下​​合闸保持弹簧"]
["拆下​​分闸线圈复位弹簧"]
["拆下合闸线圈复位弹簧"]
["拆下机构箱支撑架"]
["拆下机构合闸弹簧"]
["拆下软管"]
["拆下机构箱外壳"]
["拆下相间连杆"]
["拆下六氟化硫连接管路"]
["拆下六氟化硫密度继电器"]
["拆下阀座"]
["拆下小拐臂连杆"]
["拆下防雨罩"]
["拆下拐臂"]
["拆下A拐臂"]
["拆下C拐臂"]
["拆下固定架"]
["拆下横梁"]
["安装防爆盖"]
["安装上接线板"]
["安装静触头"]
["安装静弧触头"]
["安装泄弧剂"]
["安装绝缘拉杆"]
["安装法兰（外部端子接线端）"]
["安装灭弧室"]
["安装灭弧室瓷套"]
["安装压气缸"]
["安装下接线板"]
["安装连接轴销"]
["安装立柱瓷套下法兰"]
["安装绝缘子"]
["安装绝缘瓷套"]
["安装接线板"]
["安装静主触头"]
["安装操作箱柜门"]
["安装复位弹簧"]
["安装合闸线圈"]
["安装分闸线圈"]
["安装限位开关"]
["安装电机二次接线"]
["安装储能电机"]
["安装辅助开关"]
["安装储能凸轮"]
["安装小齿轮"]
["安装齿轮轴"]
["安装弹簧输出轴"]
["安装传动齿轮"]
["安装合闸脱扣器"]
["安装合闸掣子"]
["安装分闸掣子"]
["安装​​合闸保持弹簧"]
["安装​​分闸线圈复位弹簧"]
["安装合闸线圈复位弹簧"]
["安装机构箱支撑架"]
["安装机构合闸弹簧"]
["安装软管"]
["安装机构箱外壳"]
["安装相间连杆"]
["安装六氟化硫连接管路"]
["安装六氟化硫密度继电器"]
["安装阀座"]
["安装小拐臂连杆"]
["安装防雨罩"]
["安装拐臂"]
["安装A拐臂"]
["安装C拐臂"]
["安装固定架"]
["安装横梁"]